■ Aircraft.cfg 의 [lights] 항목을 아래 내용으로 교체

[lights]
//Types: 1=beacon, 2=strobe, 3=navigation, 4=cockpit, 5=landing
light.0 = 8, 7.7, -27, -1, tdsb8_wing_light
light.1 = 8, 7.7, 27, -1, tdsb8_wing_light
light.2 = 3, 54.787, 0, -8.5, tdsnose_gearwell
light.3 = 1, 6.0, 0, -10.5, fx_shockwave_beaconb // Beacon Below
light.4 = 1, 33.9, 0, 9.5, fx_shockwave_beaconh // Beacon Upper
light.5 = 3, -103.9, -2.8, 1.9, fx_shockwave_navwhi // Tail White L
light.6 = 3, -103.9, 2.8, 1.9, fx_shockwave_navwhi // Tail White R
light.7 = 2, -103.9, -2.8, 2.1, Fx_shockwave_strobe // Tail Strobe L
light.8 = 2, -103.9, 2.8, 2.1, Fx_shockwave_strobe // Tail Strobe R
light.9 = 5, 10.5, -11.1, -3.7, fx_shockwave_landing_light_narrow // Landing L
light.10 = 5, 10.5, 11.1, -3.7, fx_shockwave_landing_light_narrow // Landing R
light.11 = 6, 57, -0.5, -10.1, fx_shockwave_landing_light_narrow // Taxi L
light.12 = 6, 57, 0.5, -10.1, fx_shockwave_landing_light_narrow // Taxi R



■ Panel.cfg의 [VCockpit01] 항목의 마지막 줄에 아래 내용을 추가

gauge10=shockwave_lights!SW Lights_taxi_gear, 1,1,1,1 //shockwave light